ADDITION OF TWO 8 BIT

LDA 8500

MOV B, A

LDA 8501

ADD B

STA 8502

HLT

OUTPUT

