SWAPPING OF TWO 8BIT:

PROGRAM:

LDA 2500

MOV B,A

LDA 2501

STA 2500

MOV A,B

STA 2501

HLT

OUTPUT:

