8 BIT SUBTRACTION:

PROGRAM:

MVI A,20H

MVI B,10H

SUB B

STA 9000H

HLT

OUTPUT:

